**Once “BOM”**

**“DSL-rKVM19-8838TB”**

**P. O. REF. & DATE: BEPO/HD4/4000149676, Dated 27-10-2018**

**PREPARED BY CHECKED BY APPROVED BY**

**Mr. Purushotham Reddy Ms. Sabitha Rani Mr. Rajmohan.K**

**(Application Engineer) (Quality Manager) (Production Head)**

**(Datasol Rep) (Datasol Rep) (Datasol Rep.)**

| **SL NO** | **PART NO** | **PART DESCRIPTION** | **QTY / UNIT** | **MANUFACTURER or**  **SUPPLIER** | **REMARKS** |
| --- | --- | --- | --- | --- | --- |
| 1 | G190ETN01.2 | 19" display | 1 | Avnet / Advantech Local |  |
| 2 | SLP-88 | Keyboard | 1 | I KEY |  |
| 3 | TB38\_W\_BK\_65\_U | 38mm Tracker Ball | 1 | CKS |  |
| 4 | MH15-305 7nm | Hinge | 2 | REEL |  |
| 5 | LFA75F-12 | AC to DC Power Supply | 1 | COSEL |  |
| 6 | MS3102R-10SL-3P | Power Circular connector | 1 | AMPHENOL |  |
| 7 | MS3106F-10SL-3S | Power Circular matting | 1 | AMPHENOL |  |
| 8 | USB FTV 21G | USB Circular connector | 3 | AMPHENOL |  |
| 9 | EP 660-6F | Elcom Filter | 1 | ELCOM |  |
| 10 | Power Plug | 3 pin power socket with ISI Mark | 1 | CONA |  |
| 11 | USB Shielded Male to Male cable 1ft Length | USB Shielded Male to Male cable 1ft Length | 1 | STANDARD |  |
| 12 | NA | Display Control MENU Membrane Keypad | 1 | GVS ELECTRONICS |  |
| 13 | UH 275 | 2 /4 Port USB hub | 1 | ATEN |  |
| 14 | AWG 18 | Red, Black & Green wire (AWG 18) | As Per Req | PTFE |  |
| 15 | 213-0510.96--00285 | Finger Pull Handle | 2 | DIRACK |  |
| 16 | DBPL-07-GAS-01 | Gasket | 4 | SSD POLYMERS |  |
| 17 | DBPL-RKVM-07-EMI-000 | EMI Shield | 1 | SSD POLYMERS |  |
| 18 | 500 mm Length DVI-D Male to DVI-I Female cable | 500 mm Length DVI-D Male to DVI-I Female cable | 1 | PACIFIC CABLES INC. |  |
| 19 | H8550VBACA | ON /OFF Switch | 1 | ROCKER SWITCH |  |
| 20 | 657-1250F-003 | DC Feed Through Filter | 2 | API TECHNOLOGIES |  |
| 21 | 761KS17 | DC Power male Connector | 1 | SWITCHCRAFT |  |
| 22 | L712AS | DC power female connector | 1 | SWITCHCRAFT |  |
| 23 | LXR3612GD | Power LED (Green) | 1 | LUMEX |  |
| 24 | DBPL-CMF-01 | Common mode Line Filter | 1 | DATASOL |  |